Oklahoma Wind Turbine Installation Checklist (Checked if ordered/ready to ship, crossed out if delivered)

James Wang packed 3 FC to FC, 3 LC to LC, 2 e2000 to e2000, cap sets for FC and LC (no e2000)

Analyzers

~~DSS~~

~~DAS~~

LBL Luna

~~FBG~~

Workstations

~~DAS and DSS (Computer, monitor, keyboard, mouse)~~

~~FBG (Computer, monitor, keyboard, mouse)~~

Fold-up Table

Fold-up Chair

Flashlight/Lamp

Data Storage

10 T Hard drive for DAS and DSS

1 T Hard drive for FBG

1 T Hard drive for Luna

Items for the Portable Office

~~Portable Office~~

Starlink

~~UPS~~

~~FO Switch~~

~~Extension Cords~~

~~Outlets~~

Sensors and Other Related Items

Strain Cable (Red tape at the end is for the trenched cable) All others with red tape in the middle are for the longitudinal cables)

Temperature Cable

FBG Cable

~~Conduit~~

~~Patch cables fcapc e2000, and LC APC – only one e2000 – can either splice directly onto sensor cable and plug into ODH3 OR other use patch cord cables splice to FC then use FC to e2000 connector and then to e2000 – best option e2000 diamond one (ALL IN ALICIA BOX)~~

Sleeves for splices (Ask Linqing?)

Tools for splicing (Linqing to confirm, we should have for Nanzee)

~~Epoxy~~

~~Epoxy guns x2~~

~~Epoxy tips~~

PPE

~~Work Gloves~~

Work Boots (Bring from home!)

Miscellaneous

~~Gorilla Tape~~

~~Masking Tape~~

~~Rags~~